{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":6,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","5MXM-M"]
[]
[]
[]
[]
["","","","","","5MXM90M2V1B"]
["Puhallin","Ilmamäärä","Lämmitys","Erittäin pieni","cfm","851"]
["","","Jäähdytys","Erittäin pieni","cfm","851"]
["","","","Erittäin pieni","m³/min","24.1"]
["","","Jäähdytys","Erittäin pieni","m³/min","24.1"]
["Mitat","Yksikkö","","Korkeus","mm","734"]
["","","","Leveys","mm","320"]
["","","","Syvyys","mm","868"]
["Paino","Yksikkö","","","kg","68"]
["Kompressori","Tyyppi","","","","Hermeettisesti suljettu swing-kompressori"]
["Toimintalämpötila-alue","Jäähdytys","Ympäristö","Min.","°CDB","-10"]
["","","","Maks.","°CDB","46"]
["","Lämmitys","Ympäristö","Min.","°CWB","-15"]
["","","","Maks.","°CWB","18"]
["Äänenpaineen taso","Jäähdytys","","Nimell.","dBA","52"]
["","Lämmitys","","Nimell.","dBA","52"]
["Kylmäaine","Tyyppi","","","","R-32"]
["","Täytösmäärä","","","kg","2.4"]
["","Täytösmäärä","","","tCO2Eq","1.6"]
["Kylmäaine","GWP","","","","675"]
["Putkistoliitännät","Lisäkylmäainemäärä","","","kg/m","0,02 (yli 30m putkistoille)"]
["","Korkeusero","IU - OU","Maks.","m","15"]
["","","IU - IU","Maks.","m","7.5"]
["","Putkiston kokonaispituus","Järjestelmä","Todellinen","m","75"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Drain cap","","","","9"]
["","Drain plug","","","","1"]
["","Reducer assembly","","","","1"]
["","Screw bag","","","","1"]
["Virransyöttö","Vaihe","","","","1~"]
["Syöttöjännite","Syöttöjännite-=-Taajuus","","Taajuus","","50"]
["","Syöttöjännite-=-Jännite","","Jännite","","220-240"]