{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":48,"n_cols":6,"rows_kept":48,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-M"]
[]
[]
[]
[]
["","","","","","FTXM42M2V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.035"]
["","Lämmitys","","Nimell.","kW","0.035"]
["Kotelo","Väri","","","","Valkoinen"]
["Mitat","Yksikkö","","Korkeus","mm","294"]
["","","","Leveys","mm","811"]
["","","","Syvyys","mm","272"]
["Paino","Yksikkö","","","kg","10"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","12.6"]
["Puhallin","Ilmamäärä","Jäähdytys","Medium","m³/min","9.5"]
["Puhallin","Ilmamäärä","Jäähdytys","Pieni","m³/min","7.1"]
["","","","Hiljainen toiminta","m³/min","4.6"]
["","","Lämmitys","Suuri","m³/min","13"]
["Puhallin","Ilmamäärä","Lämmitys","Medium","m³/min","10.4"]
["Puhallin","Ilmamäärä","Lämmitys","Pieni","m³/min","7.1"]
["","","","Hiljainen toiminta","m³/min","5.3"]
["Äänen tehotaso","Jäähdytys","","","dBA","60"]
["","Lämmitys","","","dBA","60"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","45"]
["Äänenpaineen taso","Jäähdytys","","Keski","dBA","39"]
["Äänenpaineen taso","Jäähdytys","","Pieni","dBA","30"]
["","","","Hiljainen toiminta","dBA","21"]
["","Lämmitys","","Suuri","dBA","45"]
["","","","Keski","dBA","39"]
["","","","Pieni","dBA","29"]
["","","","Hiljainen toiminta","dBA","21"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["Putkistoliitännät","Kaasu","","Ulkohalkaisija","mm","12.7"]
["Putkiliitännät","Kondenssi","","","","18"]
["Ohjausjärjestelmät","Infrared remote control","","","","ARC466A33"]
["","Wired remote control","","","","BRC944B2, BRC073A1"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Virransyöttö","Nimi","","","","V1"]
["","Vaihe","","","","1~"]
["Syöttöjännite","Syöttöjännite-=-Taajuus","","Taajuus","","50"]
["","Syöttöjännite-=-Jännite","","Jännite","","220-240"]