{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":51,"n_cols":6,"rows_kept":51,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXG-K"]
[]
[]
[]
[]
["","","","","","FVXG35K2V1B"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.021 (1) (2) (3), 0.021 (1) (2) (3), 0.021 (1) (2) (3)"]
["","Lämmitys","","Nimell.","kW","0.024 (1) (2) (3), 0.024 (1) (2) (3), 0.024 (1) (2) (3)"]
["Kotelo","Väri","","","","Raikas valkoinen (6.5Y 9.5/0.5)"]
["Mitat","Yksikkö","","Korkeus","mm","600"]
["","","","Leveys","mm","950"]
["","","","Syvyys","mm","215"]
["Paino","Yksikkö","","","kg","22.0"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","9.1"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","7.2"]
["","","","Pieni","m³/min","5.3"]
["","","","Hiljainen toiminta","m³/min","4.5"]
["","","Lämmitys","Suuri","m³/min","10.2"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.0"]
["","","Lämmitys","Pieni","m³/min","5.8"]
["","","","Hiljainen toiminta","m³/min","5.0"]
["Äänen tehotaso","Jäähdytys","","","dBA","55"]
["","Lämmitys","","","dBA","56"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","39"]
["","","","Keski","dBA","33"]
["","","","Pieni","dBA","27"]
["","","","Hiljainen toiminta","dBA","24"]
["","Lämmitys","","Suuri","dBA","40"]
["","","","Keski","dBA","33"]
["","","","Pieni","dBA","27"]
["","","","Hiljainen toiminta","dBA","23"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Kondenssi","","","","18"]
["Ohjausjärjestelmät","Infrared remote control","","","","ARC466A2"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Installation plate","","","","1"]
["","Thermal insulation (thermal insulation tube)","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Drain hose","","","","1"]
["","Remote control holder","","","","1"]
["Virransyöttö","Nimi","","","","V1"]
["","Vaihe","","","","1~"]
["Syöttöjännite","Syöttöjännite-=-Taajuus","","Taajuus","","50"]
["","Syöttöjännite-=-Jännite","","Jännite","","220-240"]
["Huomautukset","","","","","(1) - 220 V"]
["","","","","","(2) - 230 V"]
["","","","","","(3) - 240 V"]