{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":99,"n_cols":7,"rows_kept":99,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS"]
[]
[]
[]
[]
["","","","","","FTXJ20MV1BS","FTXJ50MV1BS"]
["Äänenpaineen taso","Lämmitys","","Suuri","dBA","","47"]
["","","","Keski","dBA","","41"]
["","","","Hiljainen toiminta","dBA","","25"]
["","","","Pieni","dBA","","35"]
["","Jäähdytys","","Keski","dBA","","40"]
["","","","Hiljainen toiminta","dBA","","25"]
["","","","Pieni","dBA","","35"]
["","","","Suuri","dBA","","46"]
["Vakiovarusteet","Käyttöopas","","","","","1"]
["","Asennusohje","","","","","1"]
["","Langaton kaukosäädin","","","","","1"]
["","AAA-kuivaparistot","","","","","2"]
["","Kaukosäätimen pidike","","","","","1"]
["","Kiinnityslevyn kiinnitysruuvit","","","","","5"]
["","Kiinnityslevy","","","","","1"]
["","Raikastava titaani-apatiitti-suodatin","","","","","2"]
["","Kaukosäätimen pidikkeen kiinnitysruuvi","","","","","2"]
["","Sisäyksikön kiinnitysruuvit","","","","","2"]
["","Ruuvinsuoja","","","","","2"]
["","WLAN-sovitinsarja","","","","","1"]
["Ohjausjärjestelmät","Infrared remote control","","","","","ARC466A9"]
["Putkistoliitännät","Neste","","Ulkohalkaisija","mm","","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","","12.70"]
["","Tyhjennys","","","","","18"]
["Ottoteho","Jäähdytys","","Nimell.","kW","","0.033"]
["","Lämmitys","","Nimell.","kW","","0.043"]
["Sound power level","Jäähdytys","","","dBA","","60"]
["","Lämmitys","","","dBA","","60"]
["Mitat","Yksikkö","","Leveys","mm","","998"]
["","","","Syvyys","mm","","212"]
["","","","Korkeus","mm","","303"]
["Kotelo","Väri","","","","","Hopea"]
["Paino","Yksikkö","","","kg","","12"]
["Puhallin","Ilmamäärä","Lämmitys","Suuri","m³/min","","12.6"]
["","","","Medium","m³/min","","10.5"]
["","","","Pieni","m³/min","","8.1"]
["","","","Hiljainen toiminta","m³/min","","5.0"]
["","","Jäähdytys","Pieni","m³/min","","6.8"]
["","","","Medium","m³/min","","8.9"]
["","","","Suuri","m³/min","","10.9"]
["","","","Hiljainen toiminta","m³/min","","3.6"]
["Power supply","Vaihe","","","","","1~"]
["","Nimi","","","","","V1"]
["","Taajuus","","","Hz","","50"]
["","Jännite","","","V","","220-240"]
["Huomautukset","","","","","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V"]
["Ottoteho","Jäähdytys","","Nimell.","kW","0.023"]
["","Lämmitys","","Nimell.","kW","0.031"]
["Kotelo","Väri","","","","Hopea"]
["Mitat","Yksikkö","","Korkeus","mm","303"]
["","","","Leveys","mm","998"]
["","","","Syvyys","mm","212"]
["Paino","Yksikkö","","","kg","12"]
["Puhallin","Ilmamäärä","Jäähdytys","Suuri","m³/min","8.9"]
["","Ilman virtausnopeus","Jäähdytys","Keski","m³/min","6.6"]
["","","","Pieni","m³/min","4.4"]
["","","","Hiljainen toiminta","m³/min","2.6"]
["","","Lämmitys","Suuri","m³/min","10.2"]
["","Ilman virtausnopeus","Lämmitys","Keski","m³/min","8.4"]
["","","Lämmitys","Pieni","m³/min","6.3"]
["","","","Hiljainen toiminta","m³/min","3.8"]
["Äänen tehotaso","Jäähdytys","","","dBA","54"]
["","Lämmitys","","","dBA","56"]
["Äänenpaineen taso","Jäähdytys","","Suuri","dBA","38"]
["","","","Keski","dBA","32"]
["","","","Pieni","dBA","25"]
["","","","Hiljainen toiminta","dBA","19"]
["","Lämmitys","","Suuri","dBA","40"]
["","","","Keski","dBA","34"]
["","","","Pieni","dBA","28"]
["","","","Hiljainen toiminta","dBA","19"]
["Putkiliitännät","Neste","","Ulkohalkaisija","mm","6.35"]
["","Kaasu","","Ulkohalkaisija","mm","9.50"]
["","Kondenssi","","","","18"]
["Ohjausjärjestelmät","Infrapuna kaukosäädin","","","","ARC466A9"]
["Vakiovarusteet","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","Fixing screw for remote controller holder","","","","2"]
["","WLAN adapter kit","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Fixing screws for mounting plate","","","","5"]
["","Indoor unit fixing screws","","","","2"]
["","Mounting plate","","","","1"]
["","Remote control holder","","","","1"]
["Virransyöttö","Nimi","","","","V1"]
["","Vaihe","","","","1~"]
["Syöttöjännite","Taajuus","","","Hz","50"]
["","Jännite","","","V","220-240"]